{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet0"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet0","index":0,"n_rows":9,"n_cols":16,"rows_kept":9,"merged":[[0,0,0,15]]}
["2025年湛江市遂溪县入海排污口随机抽查情况公示表"]
["序号","计划名称","计划类型","单位名称","单位地址","企业类型","检查人名称","所属地市","所属区域","检查时间","检查情况","检查结果","状态","法定代表人","正面清单","是否发现问题"]
["1","2025年","入海排污口","遂溪县江洪镇污水处理厂入海排污口","湛江市遂溪县江洪镇","重点监管对象","何志阳,刘阳光","湛江市","遂溪县","2025-08-01 10:55:18","经检查，该厂入海排污口各项污染物排放浓度均符合相关标准要求，未发现超标排放、违规设置、监测数据造假等问题，排污行为总体规范。\n但检查中发现该厂进水氨氮指标低于设计进水浓度及常规城镇污水处理厂进水水平。进水指标过低可能影响污水处理工艺的稳定运行，降低微生物活性，长期可能导致处理效率波动等问题。\n针对上述情况，已现场提醒该厂加强进水水质监测与溯源，排查管网收集范围内是否存在雨污混接、清水混入等情况，及时采取措施优化进水水质，确保污水处理系统稳定高效运行。,经检查，该厂入海排污口各项污染物排放浓度均符合相关标准要求，未发现超标排放、违规设置、监测数据造假等问题，排污行为总体规范。\n但检查中发现该厂进水各项指标（如COD、BOD、氨氮等)均低于设计进水浓度及常规城镇污水处理厂进水水平。进水指标过低可能影响污水处理工艺的稳定运行，降低微生物活性，长期可能导致处理效率波动等问题。\n针对上述情况，已现场提醒该厂加强进水水质监测与溯源，排查管网收集范围内是否存在雨污混接、清水混入等情况，及时采取措施优化进水水质，确保污水处理系统稳定高效运行。","未发现问题终止检查并向监管对象告知检查结果","已完成","","","未发现问题"]
["2","2025年","入海排污口","遂溪旧庙养殖场4号排污口","湛江遂溪县草潭镇旧庙","一般监管对象","莫志鸿,何志阳","湛江市","遂溪县","2025-10-29 11:36:07","现场检查未发现该排口存在异常","未发现问题终止检查并向监管对象告知检查结果","已完成","","","未发现问题"]
["3","2025年","入海排污口","遂溪来路埠养殖场5号排污口","湛江市遂溪县江洪镇路埠","一般监管对象","刘阳光,莫志鸿","湛江市","遂溪县","2025-08-01 11:33:07","现场检查遂溪来路埠养殖场5号排污口排水正常无“黑臭现象”。","未发现问题终止检查并向监管对象告知检查结果","已完成","","","未发现问题"]
["4","2025年","入海排污口","遂溪红莳地养殖场1号排污口","湛江市遂溪县草潭镇","一般监管对象","何志阳,莫志鸿","湛江市","遂溪县","2025-10-29 15:18:26","现场检查未发现该排口存在环境问题","未发现问题终止检查并向监管对象告知检查结果","已完成","","","未发现问题"]
["5","2025年","入海排污口","遂溪西岭养殖场6号排污口","湛江市遂溪县界炮镇西岭","一般监管对象","刘阳光,莫志鸿","湛江市","遂溪县","2025-05-20 16:50:08","现场检查情况：现场未发现西岭养殖场排污口6号排水异常","未发现问题终止检查并向监管对象告知检查结果","已完成","","","未发现问题"]
["6","2025年","入海排污口","遂溪北灶仔养殖场6号排污口","湛江市遂溪县港门镇北灶仔","一般监管对象","何志阳,刘阳光","湛江市","遂溪县","2025-11-04 08:58:49","现场未发现异常情况","未发现问题终止检查并向监管对象告知检查结果","已完成","","","未发现问题"]
["7","2025年","入海排污口","遂溪松树埠坑养殖场1号排污口","湛江市遂溪县杨柑镇松树","一般监管对象","莫志鸿,刘阳光","湛江市","遂溪县","2025-10-29 15:11:33","现场检查未发现该排口存在异常","未发现问题终止检查并向监管对象告知检查结果","已完成","","","未发现问题"]